<?xml version="1.0" encoding="UTF-8" standalone="no"?>
<launchConfiguration type="com.pemicro.debug.gdbjtag.pne.launchConfigurationType">
  <stringAttribute key="com.pemicro.debug.gdbjtag.pne.PE.DEVICE_NAME" value="KL03Z32M4"/>
  <stringAttribute key="com.pemicro.debug.gdbjtag.pne.PE.GDB_IP" value="127.0.0.1"/>
  <stringAttribute key="com.pemicro.debug.gdbjtag.pne.PE.GDB_OPTIONS" value=""/>
  <stringAttribute key="com.pemicro.debug.gdbjtag.pne.PE.GDB_PORT" value="7224"/>
  <intAttribute key="com.pemicro.debug.gdbjtag.pne.PE.HARDWARE_INTERFACE" value="6"/>
  <stringAttribute key="com.pemicro.debug.gdbjtag.pne.PE.LAST_ATTRIBUTE_HEADER" value="com.pemicro.debug.gdbjtag.pne.sda."/>
  <booleanAttribute key="com.pemicro.debug.gdbjtag.pne.PE.USE_EXTERNAL_SERVER" value="true"/>
  <booleanAttribute key="com.pemicro.debug.gdbjtag.pne.cyc_eth.ALWAYS_ERASE" value="false"/>
  <stringAttribute key="com.pemicro.debug.gdbjtag.pne.cyc_eth.CYCLONE_IP" value=""/>
  <booleanAttribute key="com.pemicro.debug.gdbjtag.pne.cyc_eth.DO_RESET_DELAY" value="false"/>
  <intAttribute key="com.pemicro.debug.gdbjtag.pne.cyc_eth.INTERFACE_PORT" value="0"/>
  <stringAttribute key="com.pemicro.debug.gdbjtag.pne.cyc_eth.INTERFACE_PORT_STRING" value=""/>
  <stringAttribute key="com.pemicro.debug.gdbjtag.pne.cyc_eth.NETWORK_CARD_IP" value=""/>
  <stringAttribute key="com.pemicro.debug.gdbjtag.pne.cyc_eth.POWER_DOWN_DELAY" value="250"/>
  <booleanAttribute key="com.pemicro.debug.gdbjtag.pne.cyc_eth.POWER_OFF" value="false"/>
  <stringAttribute key="com.pemicro.debug.gdbjtag.pne.cyc_eth.POWER_UP_DELAY" value="250"/>
  <booleanAttribute key="com.pemicro.debug.gdbjtag.pne.cyc_eth.PROVIDE_POWER" value="false"/>
  <intAttribute key="com.pemicro.debug.gdbjtag.pne.cyc_eth.REGULATOR_VOLTAGE" value="0"/>
  <stringAttribute key="com.pemicro.debug.gdbjtag.pne.cyc_eth.RESET_DELAY" value="0"/>
  <stringAttribute key="com.pemicro.debug.gdbjtag.pne.cyc_eth.SHIFT_FREQ" value="5000"/>
  <booleanAttribute key="com.pemicro.debug.gdbjtag.pne.cyc_eth.SPECIFY_IP" value="false"/>
  <booleanAttribute key="com.pemicro.debug.gdbjtag.pne.cyc_eth.SPECIFY_NETWORK_CARD" value="false"/>
  <booleanAttribute key="com.pemicro.debug.gdbjtag.pne.cyc_eth.STARTUP_USE_SWD" value="true"/>
  <booleanAttribute key="com.pemicro.debug.gdbjtag.pne.cyc_ser.ALWAYS_ERASE" value="false"/>
  <stringAttribute key="com.pemicro.debug.gdbjtag.pne.cyc_ser.CYCLONE_IP" value=""/>
  <booleanAttribute key="com.pemicro.debug.gdbjtag.pne.cyc_ser.DO_RESET_DELAY" value="false"/>
  <intAttribute key="com.pemicro.debug.gdbjtag.pne.cyc_ser.INTERFACE_PORT" value="0"/>
  <stringAttribute key="com.pemicro.debug.gdbjtag.pne.cyc_ser.INTERFACE_PORT_STRING" value=""/>
  <stringAttribute key="com.pemicro.debug.gdbjtag.pne.cyc_ser.NETWORK_CARD_IP" value=""/>
  <stringAttribute key="com.pemicro.debug.gdbjtag.pne.cyc_ser.POWER_DOWN_DELAY" value="250"/>
  <booleanAttribute key="com.pemicro.debug.gdbjtag.pne.cyc_ser.POWER_OFF" value="false"/>
  <stringAttribute key="com.pemicro.debug.gdbjtag.pne.cyc_ser.POWER_UP_DELAY" value="250"/>
  <booleanAttribute key="com.pemicro.debug.gdbjtag.pne.cyc_ser.PROVIDE_POWER" value="false"/>
  <intAttribute key="com.pemicro.debug.gdbjtag.pne.cyc_ser.REGULATOR_VOLTAGE" value="0"/>
  <stringAttribute key="com.pemicro.debug.gdbjtag.pne.cyc_ser.RESET_DELAY" value="0"/>
  <stringAttribute key="com.pemicro.debug.gdbjtag.pne.cyc_ser.SHIFT_FREQ" value="5000"/>
  <booleanAttribute key="com.pemicro.debug.gdbjtag.pne.cyc_ser.SPECIFY_IP" value="false"/>
  <booleanAttribute key="com.pemicro.debug.gdbjtag.pne.cyc_ser.SPECIFY_NETWORK_CARD" value="false"/>
  <booleanAttribute key="com.pemicro.debug.gdbjtag.pne.cyc_ser.STARTUP_USE_SWD" value="true"/>
  <booleanAttribute key="com.pemicro.debug.gdbjtag.pne.cyc_usb.ALWAYS_ERASE" value="false"/>
  <stringAttribute key="com.pemicro.debug.gdbjtag.pne.cyc_usb.CYCLONE_IP" value=""/>
  <booleanAttribute key="com.pemicro.debug.gdbjtag.pne.cyc_usb.DO_RESET_DELAY" value="false"/>
  <intAttribute key="com.pemicro.debug.gdbjtag.pne.cyc_usb.INTERFACE_PORT" value="0"/>
  <stringAttribute key="com.pemicro.debug.gdbjtag.pne.cyc_usb.INTERFACE_PORT_STRING" value=""/>
  <stringAttribute key="com.pemicro.debug.gdbjtag.pne.cyc_usb.NETWORK_CARD_IP" value=""/>
  <stringAttribute key="com.pemicro.debug.gdbjtag.pne.cyc_usb.POWER_DOWN_DELAY" value="250"/>
  <booleanAttribute key="com.pemicro.debug.gdbjtag.pne.cyc_usb.POWER_OFF" value="false"/>
  <stringAttribute key="com.pemicro.debug.gdbjtag.pne.cyc_usb.POWER_UP_DELAY" value="250"/>
  <booleanAttribute key="com.pemicro.debug.gdbjtag.pne.cyc_usb.PROVIDE_POWER" value="false"/>
  <intAttribute key="com.pemicro.debug.gdbjtag.pne.cyc_usb.REGULATOR_VOLTAGE" value="0"/>
  <stringAttribute key="com.pemicro.debug.gdbjtag.pne.cyc_usb.RESET_DELAY" value="0"/>
  <stringAttribute key="com.pemicro.debug.gdbjtag.pne.cyc_usb.SHIFT_FREQ" value="5000"/>
  <booleanAttribute key="com.pemicro.debug.gdbjtag.pne.cyc_usb.SPECIFY_IP" value="false"/>
  <booleanAttribute key="com.pemicro.debug.gdbjtag.pne.cyc_usb.SPECIFY_NETWORK_CARD" value="false"/>
  <booleanAttribute key="com.pemicro.debug.gdbjtag.pne.cyc_usb.STARTUP_USE_SWD" value="true"/>
  <booleanAttribute key="com.pemicro.debug.gdbjtag.pne.doConnectToRunning" value="false"/>
  <booleanAttribute key="com.pemicro.debug.gdbjtag.pne.doContinue" value="true"/>
  <booleanAttribute key="com.pemicro.debug.gdbjtag.pne.doFirstReset" value="true"/>
  <booleanAttribute key="com.pemicro.debug.gdbjtag.pne.doGdbServerAllocateConsole" value="true"/>
  <booleanAttribute key="com.pemicro.debug.gdbjtag.pne.doGdbServerAllocateSemihostingConsole" value="true"/>
  <booleanAttribute key="com.pemicro.debug.gdbjtag.pne.doGdbServerInitRegs" value="true"/>
  <booleanAttribute key="com.pemicro.debug.gdbjtag.pne.doGdbServerLocalOnly" value="true"/>
  <booleanAttribute key="com.pemicro.debug.gdbjtag.pne.doGdbServerSilent" value="false"/>
  <booleanAttribute key="com.pemicro.debug.gdbjtag.pne.doGdbServerVerifyDownload" value="true"/>
  <booleanAttribute key="com.pemicro.debug.gdbjtag.pne.doSecondReset" value="true"/>
  <booleanAttribute key="com.pemicro.debug.gdbjtag.pne.doStartGdbServer" value="true"/>
  <booleanAttribute key="com.pemicro.debug.gdbjtag.pne.enableFlashBreakpoints" value="true"/>
  <booleanAttribute key="com.pemicro.debug.gdbjtag.pne.enableSemihosting" value="false"/>
  <booleanAttribute key="com.pemicro.debug.gdbjtag.pne.enableSemihostingIoclientGdbClient" value="false"/>
  <booleanAttribute key="com.pemicro.debug.gdbjtag.pne.enableSemihostingIoclientTelnet" value="false"/>
  <booleanAttribute key="com.pemicro.debug.gdbjtag.pne.enableSwo" value="true"/>
  <stringAttribute key="com.pemicro.debug.gdbjtag.pne.firstResetSpeed" value="30"/>
  <stringAttribute key="com.pemicro.debug.gdbjtag.pne.firstResetType" value=""/>
  <stringAttribute key="com.pemicro.debug.gdbjtag.pne.gdbClientOtherCommands" value="set mem inaccessible-by-default off&#13;&#10;set tcp auto-retry on&#13;&#10;set tcp connect-timeout 30"/>
  <stringAttribute key="com.pemicro.debug.gdbjtag.pne.gdbClientOtherOptions" value=""/>
  <stringAttribute key="com.pemicro.debug.gdbjtag.pne.gdbServerConnection" value="usb"/>
  <stringAttribute key="com.pemicro.debug.gdbjtag.pne.gdbServerConnectionAddress" value=""/>
  <stringAttribute key="com.pemicro.debug.gdbjtag.pne.gdbServerDebugInterface" value="swd"/>
  <stringAttribute key="com.pemicro.debug.gdbjtag.pne.gdbServerDeviceEndianness" value="little"/>
  <stringAttribute key="com.pemicro.debug.gdbjtag.pne.gdbServerDeviceName" value=""/>
  <stringAttribute key="com.pemicro.debug.gdbjtag.pne.gdbServerDeviceSpeed" value="30"/>
  <stringAttribute key="com.pemicro.debug.gdbjtag.pne.gdbServerExecutable" value="${jlink_path}/JLinkGDBServerCL"/>
  <intAttribute key="com.pemicro.debug.gdbjtag.pne.gdbServerGdbPortNumber" value="7224"/>
  <stringAttribute key="com.pemicro.debug.gdbjtag.pne.gdbServerLog" value=""/>
  <stringAttribute key="com.pemicro.debug.gdbjtag.pne.gdbServerOther" value="-s"/>
  <intAttribute key="com.pemicro.debug.gdbjtag.pne.gdbServerSwoPortNumber" value="2332"/>
  <intAttribute key="com.pemicro.debug.gdbjtag.pne.gdbServerTelnetPortNumber" value="51794"/>
  <stringAttribute key="com.pemicro.debug.gdbjtag.pne.interfaceSpeed" value="auto"/>
  <booleanAttribute key="com.pemicro.debug.gdbjtag.pne.ml.ALWAYS_ERASE" value="false"/>
  <stringAttribute key="com.pemicro.debug.gdbjtag.pne.ml.CYCLONE_IP" value=""/>
  <booleanAttribute key="com.pemicro.debug.gdbjtag.pne.ml.DO_RESET_DELAY" value="false"/>
  <intAttribute key="com.pemicro.debug.gdbjtag.pne.ml.INTERFACE_PORT" value="-1"/>
  <stringAttribute key="com.pemicro.debug.gdbjtag.pne.ml.INTERFACE_PORT_STRING" value=""/>
  <stringAttribute key="com.pemicro.debug.gdbjtag.pne.ml.NETWORK_CARD_IP" value=""/>
  <stringAttribute key="com.pemicro.debug.gdbjtag.pne.ml.POWER_DOWN_DELAY" value="250"/>
  <booleanAttribute key="com.pemicro.debug.gdbjtag.pne.ml.POWER_OFF" value="false"/>
  <stringAttribute key="com.pemicro.debug.gdbjtag.pne.ml.POWER_UP_DELAY" value="1000"/>
  <booleanAttribute key="com.pemicro.debug.gdbjtag.pne.ml.PROVIDE_POWER" value="false"/>
  <intAttribute key="com.pemicro.debug.gdbjtag.pne.ml.REGULATOR_VOLTAGE" value="0"/>
  <stringAttribute key="com.pemicro.debug.gdbjtag.pne.ml.RESET_DELAY" value="0"/>
  <stringAttribute key="com.pemicro.debug.gdbjtag.pne.ml.SHIFT_FREQ" value="5000"/>
  <booleanAttribute key="com.pemicro.debug.gdbjtag.pne.ml.SPECIFY_IP" value="false"/>
  <booleanAttribute key="com.pemicro.debug.gdbjtag.pne.ml.SPECIFY_NETWORK_CARD" value="false"/>
  <booleanAttribute key="com.pemicro.debug.gdbjtag.pne.ml.STARTUP_USE_SWD" value="true"/>
  <stringAttribute key="com.pemicro.debug.gdbjtag.pne.otherInitCommands" value=""/>
  <stringAttribute key="com.pemicro.debug.gdbjtag.pne.otherRunCommands" value=""/>
  <booleanAttribute key="com.pemicro.debug.gdbjtag.pne.sda.ALWAYS_ERASE" value="false"/>
  <stringAttribute key="com.pemicro.debug.gdbjtag.pne.sda.CYCLONE_IP" value=""/>
  <booleanAttribute key="com.pemicro.debug.gdbjtag.pne.sda.DO_RESET_DELAY" value="false"/>
  <intAttribute key="com.pemicro.debug.gdbjtag.pne.sda.INTERFACE_PORT" value="0"/>
  <stringAttribute key="com.pemicro.debug.gdbjtag.pne.sda.INTERFACE_PORT_STRING" value="USB1"/>
  <stringAttribute key="com.pemicro.debug.gdbjtag.pne.sda.NETWORK_CARD_IP" value=""/>
  <stringAttribute key="com.pemicro.debug.gdbjtag.pne.sda.POWER_DOWN_DELAY" value=""/>
  <booleanAttribute key="com.pemicro.debug.gdbjtag.pne.sda.POWER_OFF" value="false"/>
  <stringAttribute key="com.pemicro.debug.gdbjtag.pne.sda.POWER_UP_DELAY" value=""/>
  <booleanAttribute key="com.pemicro.debug.gdbjtag.pne.sda.PROVIDE_POWER" value="false"/>
  <intAttribute key="com.pemicro.debug.gdbjtag.pne.sda.REGULATOR_VOLTAGE" value="0"/>
  <stringAttribute key="com.pemicro.debug.gdbjtag.pne.sda.RESET_DELAY" value="0"/>
  <stringAttribute key="com.pemicro.debug.gdbjtag.pne.sda.SHIFT_FREQ" value="5000"/>
  <booleanAttribute key="com.pemicro.debug.gdbjtag.pne.sda.SPECIFY_IP" value="false"/>
  <booleanAttribute key="com.pemicro.debug.gdbjtag.pne.sda.SPECIFY_NETWORK_CARD" value="false"/>
  <booleanAttribute key="com.pemicro.debug.gdbjtag.pne.sda.STARTUP_USE_SWD" value="true"/>
  <stringAttribute key="com.pemicro.debug.gdbjtag.pne.secondResetType" value=""/>
  <intAttribute key="com.pemicro.debug.gdbjtag.pne.swoEnableTargetCpuFreq" value="0"/>
  <stringAttribute key="com.pemicro.debug.gdbjtag.pne.swoEnableTargetPortMask" value="0x1"/>
  <intAttribute key="com.pemicro.debug.gdbjtag.pne.swoEnableTargetSwoFreq" value="0"/>
  <booleanAttribute key="com.pemicro.debug.gdbjtag.pne.trc_eth.ALWAYS_ERASE" value="false"/>
  <stringAttribute key="com.pemicro.debug.gdbjtag.pne.trc_eth.CYCLONE_IP" value=""/>
  <booleanAttribute key="com.pemicro.debug.gdbjtag.pne.trc_eth.DO_RESET_DELAY" value="false"/>
  <intAttribute key="com.pemicro.debug.gdbjtag.pne.trc_eth.INTERFACE_PORT" value="0"/>
  <stringAttribute key="com.pemicro.debug.gdbjtag.pne.trc_eth.INTERFACE_PORT_STRING" value=""/>
  <stringAttribute key="com.pemicro.debug.gdbjtag.pne.trc_eth.NETWORK_CARD_IP" value=""/>
  <stringAttribute key="com.pemicro.debug.gdbjtag.pne.trc_eth.POWER_DOWN_DELAY" value="250"/>
  <booleanAttribute key="com.pemicro.debug.gdbjtag.pne.trc_eth.POWER_OFF" value="false"/>
  <stringAttribute key="com.pemicro.debug.gdbjtag.pne.trc_eth.POWER_UP_DELAY" value="250"/>
  <booleanAttribute key="com.pemicro.debug.gdbjtag.pne.trc_eth.PROVIDE_POWER" value="false"/>
  <intAttribute key="com.pemicro.debug.gdbjtag.pne.trc_eth.REGULATOR_VOLTAGE" value="0"/>
  <stringAttribute key="com.pemicro.debug.gdbjtag.pne.trc_eth.RESET_DELAY" value="0"/>
  <stringAttribute key="com.pemicro.debug.gdbjtag.pne.trc_eth.SHIFT_FREQ" value="5000"/>
  <booleanAttribute key="com.pemicro.debug.gdbjtag.pne.trc_eth.SPECIFY_IP" value="false"/>
  <booleanAttribute key="com.pemicro.debug.gdbjtag.pne.trc_eth.SPECIFY_NETWORK_CARD" value="false"/>
  <booleanAttribute key="com.pemicro.debug.gdbjtag.pne.trc_eth.STARTUP_USE_SWD" value="true"/>
  <booleanAttribute key="com.pemicro.debug.gdbjtag.pne.trc_usb.ALWAYS_ERASE" value="false"/>
  <stringAttribute key="com.pemicro.debug.gdbjtag.pne.trc_usb.CYCLONE_IP" value=""/>
  <booleanAttribute key="com.pemicro.debug.gdbjtag.pne.trc_usb.DO_RESET_DELAY" value="false"/>
  <intAttribute key="com.pemicro.debug.gdbjtag.pne.trc_usb.INTERFACE_PORT" value="0"/>
  <stringAttribute key="com.pemicro.debug.gdbjtag.pne.trc_usb.INTERFACE_PORT_STRING" value=""/>
  <stringAttribute key="com.pemicro.debug.gdbjtag.pne.trc_usb.NETWORK_CARD_IP" value=""/>
  <stringAttribute key="com.pemicro.debug.gdbjtag.pne.trc_usb.POWER_DOWN_DELAY" value="250"/>
  <booleanAttribute key="com.pemicro.debug.gdbjtag.pne.trc_usb.POWER_OFF" value="false"/>
  <stringAttribute key="com.pemicro.debug.gdbjtag.pne.trc_usb.POWER_UP_DELAY" value="250"/>
  <booleanAttribute key="com.pemicro.debug.gdbjtag.pne.trc_usb.PROVIDE_POWER" value="false"/>
  <intAttribute key="com.pemicro.debug.gdbjtag.pne.trc_usb.REGULATOR_VOLTAGE" value="0"/>
  <stringAttribute key="com.pemicro.debug.gdbjtag.pne.trc_usb.RESET_DELAY" value="0"/>
  <stringAttribute key="com.pemicro.debug.gdbjtag.pne.trc_usb.SHIFT_FREQ" value="5000"/>
  <booleanAttribute key="com.pemicro.debug.gdbjtag.pne.trc_usb.SPECIFY_IP" value="false"/>
  <booleanAttribute key="com.pemicro.debug.gdbjtag.pne.trc_usb.SPECIFY_NETWORK_CARD" value="false"/>
  <booleanAttribute key="com.pemicro.debug.gdbjtag.pne.trc_usb.STARTUP_USE_SWD" value="true"/>
  <stringAttribute key="org.eclipse.cdt.debug.gdbjtag.core.imageFileName" value=""/>
  <stringAttribute key="org.eclipse.cdt.debug.gdbjtag.core.imageOffset" value=""/>
  <stringAttribute key="org.eclipse.cdt.debug.gdbjtag.core.ipAddress" value="127.0.0.1"/>
  <stringAttribute key="org.eclipse.cdt.debug.gdbjtag.core.jtagDevice" value="GNU ARM J-Link"/>
  <booleanAttribute key="org.eclipse.cdt.debug.gdbjtag.core.loadImage" value="true"/>
  <booleanAttribute key="org.eclipse.cdt.debug.gdbjtag.core.loadSymbols" value="true"/>
  <stringAttribute key="org.eclipse.cdt.debug.gdbjtag.core.pcRegister" value=""/>
  <intAttribute key="org.eclipse.cdt.debug.gdbjtag.core.portNumber" value="7224"/>
  <booleanAttribute key="org.eclipse.cdt.debug.gdbjtag.core.setPcRegister" value="false"/>
  <booleanAttribute key="org.eclipse.cdt.debug.gdbjtag.core.setResume" value="false"/>
  <booleanAttribute key="org.eclipse.cdt.debug.gdbjtag.core.setStopAt" value="true"/>
  <stringAttribute key="org.eclipse.cdt.debug.gdbjtag.core.stopAt" value="main"/>
  <stringAttribute key="org.eclipse.cdt.debug.gdbjtag.core.symbolsFileName" value=""/>
  <stringAttribute key="org.eclipse.cdt.debug.gdbjtag.core.symbolsOffset" value=""/>
  <booleanAttribute key="org.eclipse.cdt.debug.gdbjtag.core.useFileForImage" value="false"/>
  <booleanAttribute key="org.eclipse.cdt.debug.gdbjtag.core.useFileForSymbols" value="false"/>
  <booleanAttribute key="org.eclipse.cdt.debug.gdbjtag.core.useProjBinaryForImage" value="true"/>
  <booleanAttribute key="org.eclipse.cdt.debug.gdbjtag.core.useProjBinaryForSymbols" value="true"/>
  <booleanAttribute key="org.eclipse.cdt.debug.gdbjtag.core.useRemoteTarget" value="true"/>
  <stringAttribute key="org.eclipse.cdt.debug.mi.core.commandFactory" value="Standard (Windows)"/>
  <stringAttribute key="org.eclipse.cdt.debug.mi.core.protocol" value="mi"/>
  <booleanAttribute key="org.eclipse.cdt.debug.mi.core.verboseMode" value="false"/>
  <stringAttribute key="org.eclipse.cdt.dsf.gdb.DEBUG_NAME" value="${cross_prefix}gdb${cross_suffix}"/>
  <booleanAttribute key="org.eclipse.cdt.dsf.gdb.UPDATE_THREADLIST_ON_SUSPEND" value="false"/>
  <intAttribute key="org.eclipse.cdt.launch.ATTR_BUILD_BEFORE_LAUNCH_ATTR" value="2"/>
  <stringAttribute key="org.eclipse.cdt.launch.COREFILE_PATH" value=""/>
  <stringAttribute key="org.eclipse.cdt.launch.PROGRAM_NAME" value="release/tpm_simple_pwm_frdmkl03z.elf"/>
  <stringAttribute key="org.eclipse.cdt.launch.PROJECT_ATTR" value="tpm_simple_pwm_frdmkl03z"/>
  <booleanAttribute key="org.eclipse.cdt.launch.PROJECT_BUILD_CONFIG_AUTO_ATTR" value="true"/>
  <stringAttribute key="org.eclipse.cdt.launch.PROJECT_BUILD_CONFIG_ID_ATTR" value="ilg.gnuarmeclipse.managedbuild.cross.config.elf.debug.1792027861"/>
  <listAttribute key="org.eclipse.debug.core.MAPPED_RESOURCE_PATHS">
    <listEntry value="/tpm_simple_pwm_frdmkl03z"/>
  </listAttribute>
  <listAttribute key="org.eclipse.debug.core.MAPPED_RESOURCE_TYPES">
    <listEntry value="4"/>
  </listAttribute>
  <booleanAttribute key="org.eclipse.debug.ui.ATTR_LAUNCH_IN_BACKGROUND" value="false"/>
  <stringAttribute key="org.eclipse.dsf.launch.MEMORY_BLOCKS" value="&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot; standalone=&quot;no&quot;?&gt;&#13;&#10;&lt;memoryBlockExpressionList context=&quot;reserved-for-future-use&quot;/&gt;&#13;&#10;"/>
  <stringAttribute key="process_factory_id" value="org.eclipse.cdt.dsf.gdb.GdbProcessFactory"/>
</launchConfiguration>
