# Kinetis Bootloader: sram_init.h Source File

sram_init.h
/*
* Copyright (c) 2014, Freescale Semiconductor, Inc.
* All rights reserved.
*
* Redistribution and use in source and binary forms, with or without modification,
* are permitted provided that the following conditions are met:
*
* o Redistributions of source code must retain the above copyright notice, this list
* of conditions and the following disclaimer.
*
* o Redistributions in binary form must reproduce the above copyright notice, this
* list of conditions and the following disclaimer in the documentation and/or
* other materials provided with the distribution.
*
* o Neither the name of Freescale Semiconductor, Inc. nor the names of its
* contributors may be used to endorse or promote products derived from this
* software without specific prior written permission.
*
* THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND CONTRIBUTORS "AS IS" AND
* ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO, THE IMPLIED
* WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE ARE
* DISCLAIMED. IN NO EVENT SHALL THE COPYRIGHT HOLDER OR CONTRIBUTORS BE LIABLE FOR
* ANY DIRECT, INDIRECT, INCIDENTAL, SPECIAL, EXEMPLARY, OR CONSEQUENTIAL DAMAGES
* (INCLUDING, BUT NOT LIMITED TO, PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES;
* LOSS OF USE, DATA, OR PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED AND ON
* ANY THEORY OF LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT
* (INCLUDING NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE OF THIS
* SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.
*/
#ifndef __SRAM_INIT_H__
#define __SRAM_INIT_H__
#include <stdint.h>
#include "memory/memory.h"
// Declarations
enum _kl_serials_sram_constants
{
kMaxRamIndex = 7,
kMinKlRamSize = (uint32_t)512
};
#if defined(__CORE_CM4_H_GENERIC) || defined(__CORE_CM7_H_GENERIC)
enum _k_serials_sram_index_constants
{
kRamSize16kIndex = 3,
kRamSize24kIndex = 4,
kRamSize32kIndex = 5,
kRamSize48kIndex = 6,
kRamSize64kIndex = 7,
kRamSize96kIndex = 8,
kRamSize128kIndex = 9,
kRamSize256kIndex = 11
};
#endif
#if defined(__CORE_CM0PLUS_H_GENERIC)
enum _k_serials_sram_index_constants
{
kRamSize0p5kIndex = 0,
kRamSize1kIndex = 1,
kRamSize2kIndex = 2,
kRamSize4kIndex = 3,
kRamSize8kIndex = 4,
kRamSize16kIndex = 5,
kRamSize32kIndex = 6,
kRamSize64kIndex = 7
};
#endif
// Prototypes
#if defined(__cplusplus)
extern "C" {
#endif // __cplusplus
status_t sram_init(void);
#if defined(__cplusplus)
}
#endif // __cplusplus
#endif
// EOF
status_t
int32_t status_t
Type used for all status and error return values.
Definition: fsl_common.h:121