# Kinetis Bootloader: smc.h Source File

smc.h
/*
* Copyright (c) 2013-14, Freescale Semiconductor, Inc.
* All rights reserved.
*
* Redistribution and use in source and binary forms, with or without modification,
* are permitted provided that the following conditions are met:
*
* o Redistributions of source code must retain the above copyright notice, this list
* of conditions and the following disclaimer.
*
* o Redistributions in binary form must reproduce the above copyright notice, this
* list of conditions and the following disclaimer in the documentation and/or
* other materials provided with the distribution.
*
* o Neither the name of Freescale Semiconductor, Inc. nor the names of its
* contributors may be used to endorse or promote products derived from this
* software without specific prior written permission.
*
* THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND CONTRIBUTORS "AS IS" AND
* ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO, THE IMPLIED
* WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE ARE
* DISCLAIMED. IN NO EVENT SHALL THE COPYRIGHT HOLDER OR CONTRIBUTORS BE LIABLE FOR
* ANY DIRECT, INDIRECT, INCIDENTAL, SPECIAL, EXEMPLARY, OR CONSEQUENTIAL DAMAGES
* (INCLUDING, BUT NOT LIMITED TO, PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES;
* LOSS OF USE, DATA, OR PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED AND ON
* ANY THEORY OF LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT
* (INCLUDING NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE OF THIS
* SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.
*/
/*
* File: smc.h
* Purpose: Provides low power mode entry routines
*
* Notes:
*/
#ifndef __SMC_H__
#define __SMC_H__
/********************************************************************/
// function prototypes
void sleep(void);
void deepsleep(void);
void enter_wait(void);
void enter_stop(uint8_t partial_stop_opt);
int32_t enter_vlpr(void);
void exit_vlpr(void);
void enter_vlps(void);
#if !defined(CPU_PKE18F512VLH15)
void enter_lls(void);
void enter_vlls3(void);
void enter_vlls2(void);
void enter_vlls1(void);
#endif
void enter_vlls0(uint8_t PORPO_value);
void enter_vlls0_nopor(void);
/********************************************************************/
#endif /* __SMC_H__ */