# Kinetis Bootloader: target_config.h Source File

validation/embedded_host/MK65F18/src/target_config.h
/*
* Copyright (c) 2014, Freescale Semiconductor, Inc.
* All rights reserved.
*
* Redistribution and use in source and binary forms, with or without modification,
* are permitted provided that the following conditions are met:
*
* o Redistributions of source code must retain the above copyright notice, this list
* of conditions and the following disclaimer.
*
* o Redistributions in binary form must reproduce the above copyright notice, this
* list of conditions and the following disclaimer in the documentation and/or
* other materials provided with the distribution.
*
* o Neither the name of Freescale Semiconductor, Inc. nor the names of its
* contributors may be used to endorse or promote products derived from this
* software without specific prior written permission.
*
* THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND CONTRIBUTORS "AS IS" AND
* ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO, THE IMPLIED
* WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE ARE
* DISCLAIMED. IN NO EVENT SHALL THE COPYRIGHT HOLDER OR CONTRIBUTORS BE LIABLE FOR
* ANY DIRECT, INDIRECT, INCIDENTAL, SPECIAL, EXEMPLARY, OR CONSEQUENTIAL DAMAGES
* (INCLUDING, BUT NOT LIMITED TO, PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES;
* LOSS OF USE, DATA, OR PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED AND ON
* ANY THEORY OF LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT
* (INCLUDING NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE OF THIS
* SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.
*/
#if !defined(__TARGET_CONFIG_H__)
#define __TARGET_CONFIG_H__
/*******************************************************************************
* Definitions
******************************************************************************/
enum _target_clocks
{
kDefaultClock = 20971520u,
kMcgOutWithFullSpeedUsb = 48000000u,
kMcgOutWithHighSpeedUsb = 120000000u,
kMinCoreClockWithFsUsbSupport = 20000000u,
kMaxCoreClock = 180000000u,
kMaxBusClock = 60000000u,
kMaxFlexBusClock = 60000000u,
kMaxFlashClock = 28000000u,
kDivider_Min = 1,
kDivider_Max = 16,
};
enum _sram_partition
{
kSram_LowerPart = 1,
kSram_UpperPart = 3,
};
enum _target_version_constants
{
kTarget_Version_Name = 'T',
kTarget_Version_Major = 1,
kTarget_Version_Minor = 0,
kTarget_Version_Bugfix = 0
};
#endif // __TARGET_CONFIG_H__